Specification for HYUNDAI DHY22KSEM

27.5kVA Single Phase Standby Diesel Generator

|  |  |
| --- | --- |
| Hyundai Backup Generator | Control Panel for Hyundai Diesel Generator |

|  |  |
| --- | --- |
| **POWER OUTPUT** | Prime Power 20kW/25kVA Stand By 22kW/27.5kVA |
| **Rpm** | 1500 |
| **ENGINE DISPLACEMENT CC** | 3298cc |
| **ENGINE MAKE** | Hyundai |
| **ENGINE TYPE** | HY4100, 4 Cylinder |
| **FUEL TANK CAPACITY** | 93 Litres |
| **FUEL TYPE** | Diesel |
| **NOISE LEVEL IN DB(A)** | 65dB(A) @ 7m |
| **Voltage @50Hz** | 240 |
| **START** | Electric |
| **RUN TIME** | 21 Hours @ 50% Load |
| **connection method** | Hardwire / 1 x 32Amp 1 x 15Amp IP67 Outlets |
| **Warranty** | 1 Year |
| **DIMENSIONS** | 2200 x 950 x 1240 mm |
| **WEIGHT** | 870kg |
| **COMES WITH** | User Manual |